static.wifi.1.security\_mode = {$yealink\_wifi\_1\_security\_mode}

static.wifi.1.cipher\_type = {$yealink\_wifi\_1\_cipher\_type}

static.wifi.1.password = {$yealink\_wifi\_1\_password\_}

static.wifi.1.eap\_type = {$yealink\_wifi\_1\_eap\_type}

static.wifi.1.eap\_user\_name = {$yealink\_wifi\_1\_eap\_user\_name}

static.wifi.1.eap\_password = {$yealink\_wifi\_1\_eap\_password}

static.wifi.show\_scan\_prompt = {$yealink\_wifi\_show\_scan\_prompt}

voice.echo\_cancellation = {$yealink\_voice\_lec}

voice.vad = {$yealink\_voice\_vad}

voice.cng = {$yealink\_voice\_cng}

account.2.sip\_server.2.port= {$sip\_port\_2}

account.1.codec.5.enable = 0

account.1.codec.5.payload\_type = G729

account.1.codec.5.priority = 0

account.1.codec.5.rtpmap = 18

account.1.codec.6.enable = 1

account.1.codec.6.payload\_type = G722

account.1.codec.6.priority = 1

remote\_phonebook.data.1.url = http://{if isset($http\_auth\_username)}{$http\_auth\_username}:{$http\_auth\_password}@{/if}{$domain\_name}/app/provision/?file=directory.xml&contacts=users

{/if}

remote\_phonebook.data.2.url = http://{if isset($http\_auth\_username)}{$http\_auth\_username}:{$http\_auth\_password}@{/if}{$domain\_name}/app/provision/?file=directory.xml&contacts=groups

{/if}

remote\_phonebook.data.3.url = http://{if isset($http\_auth\_username)}{$http\_auth\_username}:{$http\_auth\_password}@{/if}{$domain\_name}/app/provision/?file=directory.xml&contacts=extensions

{/if}

directory\_setting.url = http://{if isset($http\_auth\_username)}{$http\_auth\_username}:{$http\_auth\_password}@{/if}{$domain\_name}/app/provision/?file=favorite\_setting.xml

features.config\_dsskey\_length =